; ds600.INF
;
; INF file for the DS600 Driver
;
; 

[Version]
Signature="$Windows NT$"
Provider=%Das%
LayoutFile=ntprint.inf
ClassGUID={4D36E979-E325-11CE-BFC1-08002BE10318}
Class=Printer
CatalogFile=ptrR600.cat
DriverVer=04/18/2018,2.107.0.4
;
; Manufacturer section.
;
; This section lists all of the manufacturers 
; that we will display in the Dialog box
;
[Manufacturer]
%Das%=DAS,NTamd64

;
; Model sections. 
; 
; Each section here corresponds with an entry listed in the
; [Manufacturer] section, above. The models will be displayed in the order
; that they appear in the INF file.
;

[DAS]
"DASCOM R600"      = BITMAP,DASCOMR6002c8e,DASCOM_R600;Device ID
"DASCOM DC-7600" = BITMAP_DC7600,DASCOMDC-76002319,DASCOM_DC-7600;Device ID
"DASCOM DC-600" = BITMAP_DC600,DASCOMDC-6003919,DASCOM_DC-600;Device ID
"DASCOM DC-610" = BITMAP_DC610,DASCOMDC-610a918,DASCOM_DC-610;Device ID
"DASCOM DC-7610" = BITMAP_DC7610,DASCOMDC-7610b318,DASCOM_DC-7610;Device ID
"DASCOM DC-630" = BITMAP_DC630,DASCOMDC-630c919,DASCOM_DC-630;Device ID


[DAS.NTamd64]
"DASCOM R600"      = BITMAP,DASCOMR6002c8e,DASCOM_R600;Device ID
"DASCOM DC-7600" = BITMAP_DC7600,DASCOMDC-76002319,DASCOM_DC-7600;Device ID
"DASCOM DC-600" = BITMAP_DC600,DASCOMDC-6003919,DASCOM_DC-600;Device ID
"DASCOM DC-610" = BITMAP_DC610,DASCOMDC-610a918,DASCOM_DC-610;Device ID
"DASCOM DC-7610" = BITMAP_DC7610,DASCOMDC-7610b318,DASCOM_DC-7610;Device ID
"DASCOM DC-630" = BITMAP_DC630,DASCOMDC-630c919,DASCOM_DC-630;Device ID

;
; Installer Sections
;
; These sections control file installation, and reference all files that
; need to be copied. The section name will be assumed to be the driver
; file, unless there is an explicit DriverFile section listed.
;

[R600_COLOR_PROFILES]
R600CLR_V2_3.icm

[BITMAP]
CopyFiles=BMP,RENDER_FILES,OTHER_FILES,@ds600.gpd, R600_COLOR_PROFILES
DataSection=BITMAP_DATA
DataFile=ds600.GPD
Include=NTPRINT.INF
Needs=UNIDRV.OEM,UNIDRV_DATA

[BITMAP_DC7600]
CopyFiles=BMP_DC7600,RENDER_FILES,OTHER_FILES,@dc7600.gpd, R600_COLOR_PROFILES
DataSection=BITMAP_DATA
DataFile=dc7600.gpd
Include=NTPRINT.INF
Needs=UNIDRV.OEM,UNIDRV_DATA

[BITMAP_DC600]
CopyFiles=BMP_DC7600,RENDER_FILES,OTHER_FILES,@dc600.gpd, R600_COLOR_PROFILES
DataSection=BITMAP_DATA
DataFile=dc600.gpd
Include=NTPRINT.INF
Needs=UNIDRV.OEM,UNIDRV_DATA

[BITMAP_DC610]
CopyFiles=BMP_DC7600,RENDER_FILES,OTHER_FILES,@dc610.gpd, R600_COLOR_PROFILES
DataSection=BITMAP_DATA
DataFile=dc610.gpd
Include=NTPRINT.INF
Needs=UNIDRV.OEM,UNIDRV_DATA

[BITMAP_DC7610]
CopyFiles=BMP_DC7600,RENDER_FILES,OTHER_FILES,@dc7610.gpd, R600_COLOR_PROFILES
DataSection=BITMAP_DATA
DataFile=dc7610.gpd
Include=NTPRINT.INF
Needs=UNIDRV.OEM,UNIDRV_DATA

[BITMAP_DC630]
CopyFiles=BMP_DC7600,RENDER_FILES,OTHER_FILES,@dc630.gpd, R600_COLOR_PROFILES
DataSection=BITMAP_DATA
DataFile=dc630.gpd
Include=NTPRINT.INF
Needs=UNIDRV.OEM,UNIDRV_DATA

; Copy Sections
;
; Lists of files that are actually copied. These sections are referenced
; from the installer sections, above. Only create a section if it contains
; two or more files (if we only copy a single file, identify it in the
; installer section, using the @filename notation) or if it's a color
; profile (since the DestinationDirs can only handle sections, and not
; individual files).
;

[BMP]
ds600.DLL
ds600.INI
ds600rc.dll
ds600ui.dll
R600 UtilityTool.exe
R600 FWUpdate.exe

[BMP_DC7600]
ds600.DLL
ds600.INI
ds600rc.dll
ds600ui.dll
R600 UtilityTool.exe
R600 FWUpdate.exe

[RENDER_FILES]
ds600fm.dll
ds600cl.dll
R600YMCK.prn

[OTHER_FILES]
ds600lm.dll
ds600sm.exe
R600StatusStr.ini
;
; Data Sections
;

; These sections contain data that is shared between devices.
;

[BITMAP_DATA]
DriverFile=UNIDRV.dll
ConfigFile=unidrvui.dll
LanguageMonitor=%DAS_MONITOR%
;
;  Location of source files not in Layout.inf.
;

[SourceDisksNames.x86]
100 = %OEMSample%,,,\2k
200 = %OEMSample%,,,

[SourceDisksNames.amd64]
100 = %OEMSample%,,,\64
200 = %OEMSample%,,,


[SourceDisksFiles]
ds600.gpd   = 100
dc7600.gpd = 100
dc600.gpd = 100
dc610.gpd = 100
dc7610.gpd = 100
dc630.gpd = 100
ds600.ini    = 200
R600YMCK.prn = 200
ds600ui.dll = 100
ds600rc.dll = 100
ds600.dll    = 100
ds600fm.dll= 100
ds600cl.dll= 100
ds600lm.dll = 100
ds600sm.exe = 100
R600 UtilityTool.exe = 100
R600 FWUpdate.exe = 100
R600StatusStr.ini = 100
R600CLR_V2_3.icm = 200

;
; Call SetupSetDirectoryId with 66000 to set the target directory at runtime
; (depending on which environment drivers are getting installed)
;

[DestinationDirs]
DefaultDestDir=66000
OTHER_FILES=66002
R600_COLOR_PROFILES=66003

;
; Localizable Strings
;
[Strings]
Das="DASCOM"
OEMSample="R600 Card Driver Disk"
DAS_MONITOR="R600 Card Driver Language Monitor,ds600lm.DLL"
